Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E G H I R S T U V

## C

CardModeASYNC - Static variable in class amlib.ccid.Reader
CardModeAT45D041 - Static variable in class amlib.ccid.Reader
CardModeAT88SC - Static variable in class amlib.ccid.Reader
CardModeAT88SC102 - Static variable in class amlib.ccid.Reader
CardModeI2C - Static variable in class amlib.ccid.Reader
CardModeINPHONE - Static variable in class amlib.ccid.Reader
CardModeSLE4428 - Static variable in class amlib.ccid.Reader
CardModeSLE4442 - Static variable in class amlib.ccid.Reader
CardModeSLE6636 - Static variable in class amlib.ccid.Reader
CCID_POWEROFF - Static variable in class amlib.ccid.Reader
CCID_POWERON - Static variable in class amlib.ccid.Reader
CCID_PROTOCOL_NA - Static variable in class amlib.ccid.Reader
CCID_PROTOCOL_T0 - Static variable in class amlib.ccid.Reader
CCID_PROTOCOL_T1 - Static variable in class amlib.ccid.Reader
close() - Method in class amlib.ccid.Reader
  To close communication with ICC.
Close() - Method in class amlib.hw.HardwareInterface
  To close hardware interface
connect() - Method in class amlib.ccid.Reader
  To connect to ICC.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E G H I R S T U V