00000000 debuglog.c:269:DebugLogSetLevel() debug level=debug
00000042 debuglog.c:298:DebugLogSetCategory() Debug options: APDU
00000530 configfile.l:245:DBGetReaderListDir() Parsing conf directory: /usr/local/etc/reader.conf.d
00000565 configfile.l:287:DBGetReaderList() Parsing conf file: /usr/local/etc/reader.conf.d/libccidtwin~
00000711 configfile.l:287:DBGetReaderList() Parsing conf file: /usr/local/etc/reader.conf.d/libccidtwin
00000808 readerfactory.c:934:RFInitializeReader() Attempting startup of Generic serial 00 00 using /usr/local/lib/pcsc/drivers/serial/libccidtwin.so
00000993 readerfactory.c:824:RFBindFunctions() Loading IFD Handler 3.0
00001034 ifdhandler.c:1751:init_driver() Driver version: 1.4.5
00001697 ifdhandler.c:1768:init_driver() LogLevel: 0x0003
00001705 ifdhandler.c:1779:init_driver() DriverOptions: 0x0000
00001831 ifdhandler.c:79:IFDHCreateChannelByName() lun: 0, device: /dev/ttyS1:AU9540
00002038 ccid_serial.c:729:OpenSerialByName() Set serial port baudrate to 38400 and correct configuration
02004132 ccid_serial.c:409:ReadChunk() Timeout! (2000 ms)
02004142 ccid_serial.c:250:ReadSerial() rv 0xFC, Got 0x00, 0x00, 0x03
02004147 ccid_serial.c:746:OpenSerialByName() SetBaudrate failed. Maybe the reader is not connected
02004210 ifdhandler.c:101:IFDHCreateChannelByName() failed
02004221 readerfactory.c:965:RFInitializeReader() Open Port 0x1 Failed (/dev/ttyS1)
02004226 readerfactory.c:275:RFAddReader() Generic serial init failed.
02004236 readerfactory.c:985:RFUnInitializeReader() Attempting shutdown of Generic serial 00 00.
02004241 readerfactory.c:861:RFUnloadReader() Unloading reader driver.
02004308 readerfactory.c:934:RFInitializeReader() Attempting startup of Generic serial 00 00 using /usr/local/lib/pcsc/drivers/serial/libccidtwin.so
02004499 readerfactory.c:824:RFBindFunctions() Loading IFD Handler 3.0
02004539 ifdhandler.c:1751:init_driver() Driver version: 1.4.5
02005181 ifdhandler.c:1768:init_driver() LogLevel: 0x0003
02005189 ifdhandler.c:1779:init_driver() DriverOptions: 0x0000
02005317 ifdhandler.c:79:IFDHCreateChannelByName() lun: 0, device: /dev/ttyS1:AU9540
02005501 ccid_serial.c:729:OpenSerialByName() Set serial port baudrate to 38400 and correct configuration
04007595 ccid_serial.c:409:ReadChunk() Timeout! (2000 ms)
04007605 ccid_serial.c:250:ReadSerial() rv 0xFC, Got 0x00, 0x00, 0x03
04007611 ccid_serial.c:746:OpenSerialByName() SetBaudrate failed. Maybe the reader is not connected
04007676 ifdhandler.c:101:IFDHCreateChannelByName() failed
04007686 readerfactory.c:965:RFInitializeReader() Open Port 0x1 Failed (/dev/ttyS1)
04007691 readerfactory.c:275:RFAddReader() Generic serial init failed.
04007697 readerfactory.c:985:RFUnInitializeReader() Attempting shutdown of Generic serial 00 00.
04007701 readerfactory.c:861:RFUnloadReader() Unloading reader driver.
04007757 pcscdaemon.c:556:main() pcsc-lite 1.7.4 daemon ready.
04011495 hotplug_libusb.c:504:HPAddHotPluggable() Adding USB device: 4:2:0
04011514 readerfactory.c:934:RFInitializeReader() Attempting startup of Alcor Micro AU9540 00 00 using /usr/local/lib/pcsc/drivers/ifd-ccid.bundle/Contents/Linux/libccid.so
04011674 readerfactory.c:824:RFBindFunctions() Loading IFD Handler 3.0
04011717 ifdhandler.c:1782:init_driver() Driver version: 1.4.5
04012443 ifdhandler.c:1799:init_driver() LogLevel: 0x0003
04012452 ifdhandler.c:1810:init_driver() DriverOptions: 0x0000
04012633 ifdhandler.c:80:IFDHCreateChannelByName() lun: 0, device: usb:058f/9540:libusb-1.0:4:2:0
04013296 ccid_usb.c:245:OpenUSBByName() ifdManufacturerString: Ludovic Rousseau (ludovic.rousseau@free.fr)
04013306 ccid_usb.c:246:OpenUSBByName() ifdProductString: Generic CCID driver
04013313 ccid_usb.c:247:OpenUSBByName() Copyright: This driver is protected by terms of the GNU Lesser General Public License version 2.1, or (at your option) any later version.
04103112 ccid_usb.c:506:OpenUSBByName() Found Vendor/Product: 058F/9540 (Alcor Micro AU9540)
04103119 ccid_usb.c:508:OpenUSBByName() Using USB bus/device: 4/2
04103965 ccid_usb.c:1043:ControlUSB() control failed (4/2): -99 Success
04104387 ccid_usb.c:981:get_data_rates() Wrong GET DATA RATES size: 251
04122926 ifdhandler.c:402:IFDHGetCapabilities() tag: 0xFB3, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
04122933 readerfactory.c:295:RFAddReader() Using the reader polling thread
04124907 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
04126908 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
04133935 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
04133955 ifdhandler.c:1163:IFDHPowerICC() action: PowerUp, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
04311971 eventhandler.c:256:EHStatusHandlerThread() powerState: POWER_STATE_POWERED
04311991 Card ATR: 3B BE 11 00 00 41 01 38 00 00 00 00 00 00 00 00 01 90 00 
04313913 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x00
04313950 ifdhandler.c:402:IFDHGetCapabilities() tag: 0xFAE, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
04313955 ifdhandler.c:490:IFDHGetCapabilities() Reader supports 1 slot(s)
04314030 hotplug_libusb.c:411:HPEstablishUSBNotifications() Driver ifd-ccid.bundle does not support IFD_GENERATE_HOTPLUG. Using active polling instead.
04314035 hotplug_libusb.c:420:HPEstablishUSBNotifications() Polling forced every 1 second(s)
09318050 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x00
09318060 ifdhandler.c:1163:IFDHPowerICC() action: PowerDown, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
09320047 eventhandler.c:446:EHStatusHandlerThread() powerState: POWER_STATE_UNPOWERED
09322803 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
36375776 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x42
36375784 eventhandler.c:325:EHStatusHandlerThread() Card Removed From Alcor Micro AU9540 00 00
40823896 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
40825894 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
40825902 ifdhandler.c:1163:IFDHPowerICC() action: PowerUp, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
41003903 eventhandler.c:372:EHStatusHandlerThread() powerState: POWER_STATE_POWERED
41003908 eventhandler.c:387:EHStatusHandlerThread() Card inserted into Alcor Micro AU9540 00 00
41003919 Card ATR: 3B BE 11 00 00 41 01 38 00 00 00 00 00 00 00 00 01 90 00 
46008037 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x00
46008047 ifdhandler.c:1163:IFDHPowerICC() action: PowerDown, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
46010035 eventhandler.c:446:EHStatusHandlerThread() powerState: POWER_STATE_UNPOWERED
46012032 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
55608294 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x42
55608302 eventhandler.c:325:EHStatusHandlerThread() Card Removed From Alcor Micro AU9540 00 00
61304447 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
61306445 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
61306453 ifdhandler.c:1163:IFDHPowerICC() action: PowerUp, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
61484477 eventhandler.c:372:EHStatusHandlerThread() powerState: POWER_STATE_POWERED
61484483 eventhandler.c:387:EHStatusHandlerThread() Card inserted into Alcor Micro AU9540 00 00
61484496 Card ATR: 3B BE 11 00 00 41 01 38 00 00 00 00 00 00 00 00 01 90 00 
65816569 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x42
65816577 eventhandler.c:446:EHStatusHandlerThread() powerState: POWER_STATE_UNPOWERED
65818565 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x42
65818571 eventhandler.c:325:EHStatusHandlerThread() Card Removed From Alcor Micro AU9540 00 00
67416611 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
67418608 ifdhandler.c:1676:IFDHICCPresence() ************Cmd Get Slot Status : 0x01
67418616 ifdhandler.c:1163:IFDHPowerICC() action: PowerUp, usb:058f/9540:libusb-1.0:4:2:0 (lun: 0)
67586641 commands.c:233:CmdPowerOn Card absent or mute
67586648 ifdhandler.c:1216:IFDHPowerICC