Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E G H I R S T U V

## G

getAtr() - Method in class amlib.ccid.Reader
  Gets the ATR bytes in hex
getAtrString() - Method in class amlib.ccid.Reader
  Gets the ATR string.
getCardStatus(byte[]) - Method in class amlib.ccid.Reader
  Gets Card Status
getCmdFailCode() - Method in class amlib.ccid.Reader
  To get the CCID slot error and slot status registers of last CCID command
getCurrentDev() - Method in class amlib.ccid.Reader
  To get the current HardwareInterface instance nested in class Reader
getHWType() - Method in class amlib.hw.HardwareInterface
  To get the Hardware type
getMaxRxPkLength() - Method in class amlib.hw.HardwareInterface
  To get maximum data length for each Rx packet.
getMaxTxPkLength() - Method in class amlib.hw.HardwareInterface
  To get maximum data length for each Tx packet.
getmDevObj() - Method in class amlib.hw.HardwareInterface
  To get the casted hardware interface instance (UsbDevice for instance)which has been stored
getProtocol(byte[]) - Method in class amlib.ccid.Reader
  To get the active protocol.
getSerialNumber(byte[], byte[]) - Method in class amlib.hw.HardwareInterface
getSN(byte[], byte[]) - Method in class amlib.ccid.Reader
  To get Serial Number.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E G H I R S T U V