Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E G H I R S T U V

## S

setLog(Context, boolean, int) - Method in class amlib.hw.HardwareInterface
  To setup configurations of Hardware debug message
setPower(int) - Method in class amlib.ccid.Reader
  To set Card Power
setSlot(byte) - Method in class amlib.ccid.Reader
  To set the slot number of Reader
SLOT_STATUS_CARD_ABSENT - Static variable in class amlib.ccid.Reader
SLOT_STATUS_CARD_ACTIVE - Static variable in class amlib.ccid.Reader
SLOT_STATUS_CARD_INACTIVE - Static variable in class amlib.ccid.Reader
switchMode(byte) - Method in class amlib.ccid.Reader
  To switch to different card mode

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E G H I R S T U V