Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package amlib.ccid

It provides classes to communicating with AlcorMicro smart card reader on Android 3.1 or above.

See:
Description

Class Summary
Error |
Reader |

## Package amlib.ccid Description

It provides classes to communicating with AlcorMicro smart card reader on Android 3.1 or above.
To create Reader object
Object HardwareInterface is needed when constructing a class Reader,
you should create and initial 'HardwareInterface myDev' before create Reader

      Reader myReader

      try {
          mReader = new Reader(myDev);
      }
      catch(Exception e){
           e.printStackTrace();
      }

To connect to Reader object

      int status;
      try {
           status = mReader.connect();
       }
       catch(Exception e){
           e.printStackTrace();
      }

To power on/power off ICC

      int status;
      try {
           status = mReader.setPower(Reader.CCID_POWERON );
       }
       catch(Exception e){
           e.printStackTrace();
      }
      try {
           status = mReader.setPower(Reader.CCID_POWEROFF );
       }
       catch(Exception e){
           e.printStackTrace();
      }

Transmitting APDU

      byte pSendAPDU[] = new byte[] {(byte) 0xA0, (byte) 0xA4, 0x00, 0x00, 0x02, 0x3F, 0x00};
      byte pRxBuff[] = new byte [128];
      int pRxLen[] = new int[1];
      int status;
      try{
          status = mReader.transmit(pSendAPDU, pSendAPDU.legnth, pRxBuff, pRxLen);
          if (status != error.READER_SUCCESSFUL){
                //shows error
          }
          else{
                     for (int i=0;i<pRxLen[0]; i++){
                          Log.d(TAG, "Received byte["+ i+ "]=0x"+ Integer.toHexString(pRxBuff[i]));
                     }
          }
      }
      catch (Exception e){
               e.printStackTrace();
      }

Send Escape

      byte pData[] = new byte[] {CMD_VENDOR_OP_CODE, VENDOR_CMD, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00};
      byte pRxBuff[] = new byte [128];
      int pRxLen[] = new int[1];
      int status;
      try{
          status = mReader.escape(pData, pData.legnth, pRxBuff, pRxLen);
          if (status != error.READER_SUCCESSFUL){
                    //shows error
               }
               else{
                for (int i=0;i<pRxLen[0]; i++){
                    Log.d(TAG, "Received byte["+ i+ "]=0x"+ Integer.toHexString(pRxBuff[i]));
                 }
           }
      }
     catch (Exception e){
               e.printStackTrace();
     }

To get ATR

      String atr;
      byte []atrArray = new byte[64];
      try {
          atr = mReader.getAtrString();
          atrArray = mReader.getAtr();
      }
      catch (Exception e){
               e.printStackTrace();
      }

To get Card Status

     byte pCardStatus[] = new byte[1];
     int status;
     try {
           status = mReader.getCardStatus(pCardStatus);
       }
       catch(Exception e){
           e.printStackTrace();
       }
       if (status == error.READER_SUCCESSFUL){
           //shows card status
       }

To get current protcol

        byte []proto = new byte[1];
        try {
            status = mReader.getProtocol(proto);
        }
        catch(Exception e){
            e.printStackTrace();
        }

        if (status == error.READER_SUCCESSFUL && proto[0] == Reader.CCID_PROTOCOL_T0){
            //do something
        }

To get SN in EEPROM

        byte pLen[] = new byte[1];
        byte []pSN;
        pLen[0] = 32;
        pSN = new byte[pLen[0]];
        try {
            status = mReader.getSN(pSN, pLen);
        }
        catch(Exception e){
            e.printStackTrace();
        }
        if (status == error.READER_SUCCESSFUL){
            //shows the SN
        }

To close Reader

      try {
            if (myDev.Close()){
                 //shows error
            }
        }
        catch(Exception e){
            e.printStackTrace();
        }

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES